{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["Risico-inventarisatie","Risicograaf","Blad1","Lijsten"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":6,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Risico-inventarisatie","index":0,"n_rows":21,"n_cols":10,"rows_kept":21,"cut":false,"hidden":false,"merged":[[19,1,19,4],[20,1,20,4],[21,1,21,4],[22,1,22,4],[23,1,23,4],[14,1,14,4],[15,1,15,4],[16,1,16,4],[17,1,17,4],[18,1,18,4],[3,1,3,4],[4,1,4,4],[5,1,5,4],[6,1,6,4],[7,1,7,4],[8,1,8,4],[9,1,9,4],[10,1,10,4],[11,1,11,4],[12,1,12,4],[13,1,13,4],[30,1,30,4],[31,1,31,4],[32,1,32,4],[25,1,25,4],[26,1,26,4],[27,1,27,4],[28,1,28,4],[29,1,29,4],[24,1,24,4],[2,1,2,4],[1,1,1,4]]}
[null,"Machine: ","TEST"]
["Voorbeelden ","Mechanische gevaren ",null,null,null,"Volgnummer","Ernst","Blootstelling","Waarschijnlijkheid","Risico-index"]
["versnelling/vertraging","Beknelling tijdens zakken ",null,null,null,1,1,0.5,0.1,{"$f":"G3*H3*I3","v":0.05}]
["puntige delen",null,null,null,null,2,1,0.5,0.1,{"$f":"G4*H4*I4","v":0.05}]
["nadering bewegend element tot een vast deel",null,null,null,null,3,1,0.5,0.1,{"$f":"G5*H5*I5","v":0.05}]
["snijdende-verspanende delen ",null,null,null,null,4,1,0.5,0.1,{"$f":"G6*H6*I6","v":0.05}]
["verende/elastische delen",null,null,null,null,5,1,0.5,0.1,{"$f":"G7*H7*I7","v":0.05}]
["vallende delen/voorwerpen ",null,null,null,null,6,1,0.5,0.1,{"$f":"G8*H8*I8","v":0.05}]
["zwaartekracht",null,null,null,null,7,1,0.5,0.1,{"$f":"G9*H9*I9","v":0.05}]
["hoogte",null,null,null,null,8,1,0.5,0.1,{"$f":"G10*H10*I10","v":0.05}]
["hoge druk ",null,null,null,null,9,1,0.5,0.1,{"$f":"G11*H11*I11","v":0.05}]
["instabiliteit ",null,null,null,null,10,1,0.5,0.1,{"$f":"G12*H12*I12","v":0.05}]
["kinetische energie ",null,null,null,null,11,1,0.5,0.1,{"$f":"G13*H13*I13","v":0.05}]
["beweging van de machine(s)",null,null,null,null,12,1,0.5,0.1,{"$f":"G14*H14*I14","v":0.05}]
["bewegende delen",null,null,null,null,13,1,0.5,0.1,{"$f":"G15*H15*I15","v":0.05}]
["draaiende delen ",null,null,null,null,14,1,0.5,0.1,{"$f":"G16*H16*I16","v":0.05}]
["ruw oppervlak",null,null,null,null,15,1,0.5,0.1,{"$f":"G17*H17*I17","v":0.05}]
["glad oppervlak "]
["scherpe kanten"]
["opgeslagen energie"]
["vacuüm"]

{"sheet":"Risicograaf","index":1,"n_rows":14,"n_cols":3,"rows_kept":14,"cut":false,"hidden":false,"merged":[]}
["E (ernst van het effect)","B (blootstelling)","W (waarschijnlijkheid, kans)"]
["100 catastrofaal, vele doden","10    voortdurend","10     kan worden verwacht, bijna zeker"]
[" 40 ramp, verscheidene doden"," 6    dagelijks tijdens werkuren","   6    goed mogelijk"]
[" 15 zeer ernstig, één dode"," 3    wekelijks of incidenteel","   3    ongewoon, maar mogelijk"]
["    7 aanzienlijk, blijvend letsel"," 2    maandelijks"," 0,5 onwaarschijnlijk"]
["    3 tijdelijke arbeidsongeschiktheid"," 1    enkele malen per jaar"," 0,2 vrijwel onmogelijk"]
["    1 betekenisvol, EHBO vereist"," 0,5 zeer zelden"," 0,1 bijna niet denkbaar"]
[]
["Klasse","Risicoscore","Prioriteit"]
[1,"R ≤20","Geen prioriteit (aanvaardbaar risico)"]
[2,"20 < R ≤70","Aandacht vereist (enig of mogelijk risico)"]
[3,"70 < R ≤200","Maatregelen vereist (belangrijk risico)"]
[4,"200 < R ≤400","Directe verbetering vereist (hoog risico)"]
[5,"R > 400","Werkzaamheden stoppen (zeer hoog risico)"]

{"sheet":"Blad1","index":2,"n_rows":19,"n_cols":12,"rows_kept":19,"cut":false,"hidden":false,"merged":[[11,0,11,11],[12,0,12,9],[12,10,12,11],[21,0,21,11],[13,0,13,11],[15,0,16,6],[17,0,17,11],[19,0,20,6],[19,7,20,11],[18,7,18,11],[18,0,18,6],[0,1,0,6],[0,7,0,8],[0,9,0,11],[1,1,1,11],[2,1,2,11],[3,0,3,11],[14,7,15,7],[14,8,15,8],[14,9,15,9],[14,10,15,10],[14,11,15,11],[14,0,14,6],[4,0,4,6],[5,0,5,6],[6,0,6,11],[7,0,7,11],[8,0,8,9],[8,10,8,11],[9,0,9,11],[10,0,10,9],[10,10,10,11]]}
["Machine ",{"$f":"Machine","v":"TEST"},null,null,null,null,null,"Volgnummer: "]
["Machinedeel "]
["Datum "]
[]
["Risicobeoordeling:",null,null,null,null,null,null,"Fase","Ernst","Bloot stelling","Waarschijn-lijkheid","Kans"]
[null,null,null,null,null,null,null,"Norm. Bedr. ",3,10,0.5,{"$f":"I6*J6*K6","v":15}]
[]
["Risco: Letsel door gevaar/omstandigheid/gebeurtenis/omgeving"]
[]
["Advies: Risicoreductie: Constructief - Afscherming - Waarschuwing "]
[]
["Uitvoering risicoreductie:"]
[]
[]
["Overblijvend risico: ",null,null,null,null,null,null,"Fase","Ernst","Bloot stelling","Waarschijn-lijkheid","Kans"]
[]
[null,null,null,null,null,null,null,"Norm. Bedr. ",3,10,0.5,{"$f":"I17*J17*K17","v":15}]
[]
["Omschrijving restrisico ",null,null,null,null,null,null,"Actie"]

{"sheet":"Lijsten","index":3,"n_rows":7,"n_cols":6,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["Ernst",null,"Blootstelling",null,"Waarschijnlijkheid"]
["catastrofaal, vele doden",100,"voortdurend",10,"kan worden verwacht, bijna zeker",10]
["ramp, verscheidene doden",40,"dagelijks tijdens werkuren",6,"goed mogelijk",6]
["zeer ernstig, één dode",15,"wekelijks of incidenteel",3,"ongewoon, maar mogelijk",3]
["aanzienlijk, blijvend letsel",7,"maandelijks",2,"onwaarschijnlijk",0.5]
["tijdelijke arbeidsongeschiktheid",3,"enkele malen per jaar",1,"vrijwel onmogelijk",0.2]
["betekenisvol, EHBO vereist",1,"zeer zelden",0.5,"bijna niet denkbaar",0.1]