{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Hoe het is"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Hoe het is","index":0,"n_rows":69,"n_cols":3,"rows_kept":69,"cut":false,"hidden":false,"merged":[]}
["hoofdgroep","groep","subgroep"]
["gyproc","platen","ABA 9,5mm"]
["gyproc","platen","ABA 9,5mm"]
["gyproc","platen","ABA 12,5mm"]
["gyproc","platen","ABA 12,5mm"]
["gyproc","platen","ABA 12,5mm"]
["gyproc","platen","ABA 12,5mm"]
["gyproc","platen","WR ABA 12,5mm"]
["gyproc","platen","WR ABA 12,5mm"]
["gyproc","platen","WR 4xABA 12,5mm"]
["gyproc","platen","WR 4xABA 12,5mm"]
["gyproc","platen","Activ'Air Premium ABA 12,5mm"]
["gyproc","platen","Activ'Air Premium 4xABA 12,5mm"]
["gyproc","platen","Activ'Air Premium 4xABA 12,5mm"]
["gyproc","platen","RF ABA 12,5mm"]
["gyproc","platen","RF ABA 15mm"]
["gyproc","platen","RF 4xABA 15mm"]
["gyproc","platen","RF ABA 18mm"]
["gyproc","afwerking","flex corner"]
["gyproc","afwerking","easy flex pro"]
["gyproc","afwerking","Corner bead"]
["gyproc","afwerking","Aqua Bead buitenhoek"]
["gyproc","afwerking","Aqua bead Flex Pro"]
["gyproc","afwerking","Corner Arch"]
["gyproc","afwerking","Metal edge trim"]
["gyproc","afwerking","Board Stop"]
["gyproc","afwerking","kooflijst Mini"]
["gyproc","bevestiging","schroef"]
["gyproc","bevestiging","schroef"]
["gyproc","bevestiging","schroef"]
["gyproc","bevestiging","schroef"]
["gyproc","inspectieluik","Prolock Alu Standaard"]
["gyproc","inspectieluik","Prolock Alu Standaard"]
["gyproc","inspectieluik","Prolock Alu Standaard"]
["gyproc","Metal Stud","50mm Horizontaal"]
["gyproc","Metal Stud","50mm Verticaal"]
["gyproc","Metal Stud","50mm Verticaal"]
["gyproc","Metal Stud","50mm Verticaal"]
["gyproc","Metal Stud","75mm Horizontaal"]
["gyproc","Metal Stud","75mm Verticaal"]
["gyproc","Metal Stud","75mm Verticaal"]
["gyproc","Metal Stud","75mm Verticaal"]
["gyproc","Metal Stud","100mm Horizontaal"]
["gyproc","Metal Stud","100mm Verticaal"]
["gyproc","Metal Stud","100mm Verticaal"]
["gyproc","Metal Stud","isolatieband"]
["gyproc","Metal Stud","isolatieband"]
["Fermacell","4 ABA","10mm"]
["Fermacell","Rechte Boord","10mm"]
["Fermacell","Rechte Boord","10mm"]
["Fermacell","Rechte Boord","12,5mm"]
["Fermacell","Rechte Boord","12,5mm"]
["Fermacell","finisch Kant-en-klaar"]
["Fermacell","finisch Kant-en-klaar"]
["Fermacell","gipslijm"]
["Fermacell","voegenlijm"]
["Fermacell","schroeven"]
["Fermacell","platenvoorsnijmes"]
["Fermacell","vloerelement","20mm (2E 11)"]
["Fermacell","vloerelement","20mm+10mm MW (2E 32)"]
["Fermacell","droge egalisatiekorrels"]
["Fermacell","montagelijm"]
["Fermacell","schroeven"]
["Fermacell","randstrook","30mm"]
["Hydropanel","2 x afgeschuind","9mm"]
["Hydropanel","3 x afgeschuind","9mm"]
["Hydropanel","schroef"]
["Hydropanel","primer"]
["Hydropanel","Finisher"]