{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["BOM"],"not_rendered":{"charts":0,"images":260,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BOM","index":0,"n_rows":701,"n_cols":6,"rows_kept":701,"cut":false,"hidden":false,"merged":[]}
["QTY","Part Number","Title","Description","Thumbnail","Mass"]
[1,"518679CC","BOVENBAND CC.142-501420CC",null,null,"3998,937 kg"]
[1,null,"E-KAST 500x500x210 (CONTROLS)","E-KAST 500x500x210 (CONTROLS)",null,"15,591 kg"]
[4,221040,"M8*50; RVS ZK.TAPBOUT; A2","M8*50; RVS ZK.TAPBOUT; A2",null,"0,003 kg"]
[4,"223005","M8; ZK.MOER; RVS; A2","M8; ZK.MOER; RVS; A2",null,"0,005 kg"]
[1,225005,"M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[1,"E-KAST RITTAL AE 1007.600 (500-500-210)","RITTAL AE 1007.600 (500*500*210)","RITTAL AE 1007.600 (500*500*210)",null,"15,555 kg"]
[4,"221035","M8*25; ZK.TAPBOUT; RVS, A2","M8*25; ZK.TAPBOUT; RVS, A2",null,"0,016 kg"]
[8,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[8,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[6,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[12,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[10,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[4,"225057","M12; RVS VEERRING; A2; DIN127","M12; RVS VEERRING; A2; DIN127",null,"0,004 kg"]
[2,"262213-M3-270gr-3","KA77 DRN132M4; 7,5; N=99; 480; 60; M3A","KA77 DRN132M4; 7,5; N=99; 480; 60; M3A",null,"126,000 kg"]
[1,"262344-M1-0gr-X","RF07 DRN71MS4; 0.25; N=51; 480; M1","RF07 DRN71MS4; 0.25; N=51; 480; M1",null,"9,300 kg"]
[2,"262350-M1-0gr-X","RF07 DRN71MS4/BE03HR","RF07 DRN71MS4/BE03HR",null,"37,000 kg"]
[2,"262924","BUFFER MET DRAADEIND; DEMAG 233.701.045","BUFFER MET DRAADEIND; DEMAG 233.701.045",null,"0,236 kg"]
[1,"440397FS","TYPEPLAAT GTL/THILOT 160*77*3","TYPEPLAAT GTL/THILOT 160*77*3",null,"0,087 kg"]
[2,"450877CC","BEVESTINGSPLAAT BUFFER","PLAAT 240*90*10",null,"1,601 kg"]
[1,"470554CC","BEV. STEUN MEENEMER VLAKKABEL","PLAAT 242*231*3",null,"0,853 kg"]
[1,"480509CC","TR-BAND; RUB; 1400*42950; OPEN","TR-BAND; RUB; 1400*42950",null,"600,931 kg"]
[4,"516616CC","LOOPWAGEN BOVENBAND; AANGEDREVEN",null,null,"23,681 kg"]
[4,"221025","M6*30; ZK.TAPBOUT; RVS; A2","M6*30; ZK.TAPBOUT; RVS; A2",null,"0,009 kg"]
[4,"224457","M6; RVS BORGMOER; A2","M6; RVS BORGMOER; A2",null,"0,003 kg"]
[4,"225004","M6; RVS SLUITRING; A2; DIN125A","M6; RVS SLUITRING; A2; DIN125A",null,"0,001 kg"]
[1,"404055CC","TANDWIEL AANDRIJVING RIJWERK SCHUIFBAND",null,null,"0,321 kg"]
[1,"245811","TANDWIEL; Z=15; M=3; RVS","TANDWIEL; Z=15; M=3; RVS",null,"0,402 kg"]
[2,"515507CC","LOOPROL SCHUIFBAND AANGEDREVEN; KPL",null,null,"2,132 kg"]
[1,"221085","M20*50; ZK.RVS.TAPBOUT; A2","M20*50; ZK.RVS.TAPBOUT; A2",null,"0,199 kg"]
[1,"225011","M20; RVS SLUITRING; A2; DIN125A","M20; RVS SLUITRING; A2; DIN125A",null,"0,018 kg"]
[1,"225061","M20; VEERRING; RVS; A2","M20; VEERRING; RVS; A2",null,"0,013 kg"]
[1,"225425","ASBORGRING ø35; RVS","ASBORGRING ø35; RVS",null,"0,004 kg"]
[1,"225558","GATBORGRING; G72; RVS","GATBORGRING; G72; RVS",null,"0,020 kg"]
[1,"243060","KOGELLAGER 6207-2RS1; RVS KOGELLAGER","KOGELLAGER 6207-2RS1; RVS KOGELLAGER",null,"0,281 kg"]
[1,"404048CC","AS LOOPROL SCHUIFBAND","AS ø40-43",null,"0,299 kg"]
[1,"535594CC","LOOPROL SCHUIFBAND AANGEDREVEN",null,null,"1,298 kg"]
[2,"515508CC","LOOPROL SCHUIFBAND VRIJLOOP; KPL",null,null,"2,140 kg"]
[1,"221085","M20*50; ZK.RVS.TAPBOUT; A2","M20*50; ZK.RVS.TAPBOUT; A2",null,"0,199 kg"]
[1,"225011","M20; RVS SLUITRING; A2; DIN125A","M20; RVS SLUITRING; A2; DIN125A",null,"0,018 kg"]
[1,"225061","M20; VEERRING; RVS; A2","M20; VEERRING; RVS; A2",null,"0,013 kg"]
[1,"225425","ASBORGRING ø35; RVS","ASBORGRING ø35; RVS",null,"0,004 kg"]
[1,"225558","GATBORGRING; G72; RVS","GATBORGRING; G72; RVS",null,"0,020 kg"]
[1,"243060","KOGELLAGER 6207-2RS1; RVS KOGELLAGER","KOGELLAGER 6207-2RS1; RVS KOGELLAGER",null,"0,281 kg"]
[1,"404048CC","AS LOOPROL SCHUIFBAND","AS ø40-43",null,"0,299 kg"]
[1,"535595CC","LOOPROL SCHUIFBAND VRIJLOOP",null,null,"1,305 kg"]
[1,"537232CC","FRAME LOOPWAGEN CC.142; AANGEDREVEN",null,null,"14,764 kg"]
[4,"516617CC","LOOPWAGEN BOVENBAND CC.142; VRIJLOOP",null,null,"23,895 kg"]
[4,"515508CC","LOOPROL SCHUIFBAND VRIJLOOP; KPL",null,null,"2,140 kg"]
[1,"221085","M20*50; ZK.RVS.TAPBOUT; A2","M20*50; ZK.RVS.TAPBOUT; A2",null,"0,199 kg"]
[1,"225011","M20; RVS SLUITRING; A2; DIN125A","M20; RVS SLUITRING; A2; DIN125A",null,"0,018 kg"]
[1,"225061","M20; VEERRING; RVS; A2","M20; VEERRING; RVS; A2",null,"0,013 kg"]
[1,"225425","ASBORGRING ø35; RVS","ASBORGRING ø35; RVS",null,"0,004 kg"]
[1,"225558","GATBORGRING; G72; RVS","GATBORGRING; G72; RVS",null,"0,020 kg"]
[1,"243060","KOGELLAGER 6207-2RS1; RVS KOGELLAGER","KOGELLAGER 6207-2RS1; RVS KOGELLAGER",null,"0,281 kg"]
[1,"404048CC","AS LOOPROL SCHUIFBAND","AS ø40-43",null,"0,299 kg"]
[1,"535595CC","LOOPROL SCHUIFBAND VRIJLOOP",null,null,"1,305 kg"]
[1,"537231CC","FRAME LOOPWAGEN CC.142; VRIJLOOP",null,null,"15,337 kg"]
[1,"518327CC","KOPSTUK BOVENBAND CC.142; L",null,null,"1123,792 kg"]
[2,"212009","M20; THVZ DRAADEIND; ISO; 8.8","M20; THVZ DRAADEIND; ISO; 8.8",null,"2,522 kg"]
[18,"217780","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART",null,"0,020 kg"]
[8,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[8,"221046","M10*20; ZK.TAPBOUT; RVS; A2","M10*20; ZK.TAPBOUT; RVS; A2",null,"0,025 kg"]
[78,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[3,"221073","M16*40; RVS ZK. TAPBOUT; A2 DIN933","M16*40; RVS ZK. TAPBOUT; A2 DIN933",null,"0,101 kg"]
[3,"221075","M16*50; ZK TAPBOUT; RVS; A2","M16*50; ZK TAPBOUT; RVS; A2",null,"0,116 kg"]
[4,"221243","M12*60; RVS ZK. BOUT; A2; DIN931","M12*60; RVS ZK. BOUT; A2; DIN931",null,"0,071 kg"]
[19,"221247","M12*90; RVS ZK. BOUT; A2","M12*90; RVS ZK. BOUT; A2",null,"0,095 kg"]
[8,"221253","M16*60; RVS ZK. BOUT; A2; DIN931","M16*60; RVS ZK. BOUT; A2; DIN931",null,"0,136 kg"]
[3,"221257","M16*80;ZK.RVS BOUT; A2","M16*80;ZK.RVS BOUT; A2",null,"0,163 kg"]
[22,"222244","M8*35;  A2;CIL.SCHR+BINNENZESK","M8*35;  A2;CIL.SCHR+BINNENZESK",null,"0,021 kg"]
[14,"223011","M20; ZK.MOER; RVS; A2","M20; ZK.MOER; RVS; A2",null,"0,065 kg"]
[30,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[83,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[15,"224462","M16; RVS BORGMOER; A2","M16; RVS BORGMOER; A2",null,"0,037 kg"]
[42,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[180,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[21,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[8,"225024","M10; CARROS.SLUITRING; RVS; A2","M10; CARROS.SLUITRING; RVS; A2",null,"0,012 kg"]
[12,"225026","M16; CARROS. SLUITRING","M16; CARROS. SLUITRING",null,"0,042 kg"]
[8,"225028","M20; RVS SLUITRING; A2; M20*44*8;DIN7349","M20; RVS SLUITRING; A2; M20*44*8;DIN7349",null,"0,075 kg"]
[20,"225057","M12; RVS VEERRING; A2; DIN127","M12; RVS VEERRING; A2; DIN127",null,"0,004 kg"]
[2,"225059","M16; RVS VEERRING; A2","M16; RVS VEERRING; A2",null,"0,008 kg"]
[2,"243279","22212 EK; TONLAGER; SKF","22212 EK; TONLAGER; SKF",null,"1,150 kg"]
[2,"243530","SNL 512-610; LAGERHUIS; SKF","SNL 512-610; LAGERHUIS; SKF",null,"5,740 kg"]
[1,"243602","ASNH 512-610 EINDDEKSEL; SKF","ASNH 512-610 EINDDEKSEL; SKF",null,"0,120 kg"]
["1,500 ul","243632","TSNA 512 A; AFDICHTING; SKF","TSNA 512 A; AFDICHTING; SKF",null,"0,060 kg"]
["4,000 ul","243694","FRB 10/110; AFSTANDSRING; SKF","FRB 10/110; AFSTANDSRING; SKF",null,"0,246 kg"]
[2,"243702","H 312; TREKBUS; SKF","H 312; TREKBUS; SKF",null,"0,400 kg"]
[4,"246405","ZIJGELEIDEROL ø63.5*100; B","ZIJGELEIDEROL ø63.5*100; B",null,"0,998 kg"]
[11,"246416","TRANSPORTROL ø89*530; AS ø20*560","TRANSPORTROL ø89*530; AS ø20*560",null,"4,000 kg"]
[4,"246435","TRANSPORTROL ø89*1550; AS ø25*1581","TRANSPORTROL ø89*1550; AS ø25*1581",null,"16,889 kg"]
[24,"246580","TRANSPORTROL ø89*465; AS ø20*495","TRANSPORTROL ø89*465; AS ø20*495",null,"3,500 kg"]
[2,"247562","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"1,203 kg"]
[1,"247562-1","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"0,470 kg"]
[2,"247562-2","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"0,366 kg"]
[1,"400586FS","SMEERBOUT M16*40","SMEERBOUT M16*40",null,"0,099 kg"]
[1,"211804","1/8\"G-180º; SMEERNIPPEL","1/8\"G-180º; SMEERNIPPEL",null,"0,008 kg"]
[1,"400586FS","TAPBOUT THVZ. M16*40","TAPBOUT THVZ. M16*40",null,"0,092 kg"]
[1,"400591RT","BORGSCHIJF KA76; ø70*ø17*8","BORGSCHIJF KA76; ø70*ø17*8",null,"0,079 kg"]
[1,"400128RT","BORGSCHIJF ø70*ø13*8;  KA76","PLAAT ø70*8",null,"0,081 kg"]
[19,"404008TS","AFSTANDSBUS TROGSTELBEUGEL TS","BUIS ø21,3*2,65-54",null,"0,067 kg"]
[1,"405035CC","OPVULBUS ø70*ø50-20","BUIS ø70*10-20",null,"0,291 kg"]
[2,"405065TF","AS ø6-1300","AS ø6-1300",null,"0,295 kg"]
[4,"405070TF","AS ø6-3000","AS ø6-3000",null,"0,681 kg"]
[1,"405210TS","OPVULBUS ø30*ø16,5*20,5","AS ø30-20,5",null,"0,081 kg"]
[2,"406253TS","DRAADSPIL M20*750; THVZ","DRAADSPIL M20*750; THVZ",null,"1,851 kg"]
[4,"406316CC","DRAADBUS TROGSTELBEUGEL BEGIN/EIND","AS ø20-54",null,"0,101 kg"]
[1,"448547CC","RUBBER SCHRAPER DR-TROMMEL CC/TS.140","PLAAT 1500*200*6",null,"1,790 kg"]
[1,"448548CC","KLEMSTRIP RUBBER; L=1480; HOH.200","PLAAT 1480*35*3",null,"1,234 kg"]
[2,"449350CC","BORGPLAAT STORTSCHOT CC.140","PLAAT 80*65*5",null,"0,085 kg"]
[1,"450871CC","SCHUIFBLOK REACTIEARM","PLAAT 115*30*12",null,"0,136 kg"]
[2,"451866CC","TREKSTRIP SCHOOR CC.160; L=2770","PLAAT 2810*40*5",null,"4,481 kg"]
[1,"467181CC","SCHRAPER KEERTROMMEL CC/TS.140","PLAAT 1600*264*4",null,"13,204 kg"]
[1,"467185CC","SCHRAPER DRIJFTROMMEL UITW; CC/TS.140","PLAAT 1743*116*5",null,"7,632 kg"]
[8,"467187CC","STEUNROLHOUDER CC.142","PLAAT 190*136*5",null,"0,868 kg"]
[2,"467210CC","STEUN GELEIDING STORTSCHOT CC.142","PLAAT 433*79*5",null,"0,859 kg"]
[4,"467212CC","BEV.BEUGEL ZIJGELEIDEROL CC.142","PLAAT 189*65*10",null,"0,904 kg"]
[2,"467217CC","BEV.STEUN TROGSTELBEUGEL STUREN CC.142","PLAAT 160*152*8",null,"1,177 kg"]
[1,"469048CC","BEV.STEUN SCHRAPER DRIJFTR CC.142; R","PLAAT 280*267*6",null,"1,397 kg"]
[1,"469048CC_MIR","BEV.STEUN SCHRAPER DRIJFTR CC.142; L","PLAAT 280*267*6",null,"1,397 kg"]
[1,"469070CC","REACTIEARM KA77","PLAAT 858*170*10",null,"6,913 kg"]
[1,"516338CC","TROGSTELBEUGEL CC.142; 10°; STUREN; KPL",null,null,"13,965 kg"]
[4,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[4,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[4,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[2,"467226CC","KLEMPLAAT DRAAGROL STUREN CC","PLAAT 148*60*5",null,"0,097 kg"]
[1,"536754CC","TROGSTELBEUGEL CC.142; 10°; STUREN",null,null,"13,664 kg"]
[1,"516606CC","STORTSCHOT BOVENBAND CC.142; KPL",null,null,"60,918 kg"]
[2,"218001","INSTEEKDOP ø42*1.3/3","INSTEEKDOP ø42*1.3/3",null,"0,009 kg"]
[8,"221035","M8*25; ZK.TAPBOUT; RVS, A2","M8*25; ZK.TAPBOUT; RVS, A2",null,"0,016 kg"]
[8,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[8,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[8,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[8,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[16,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[8,"225023","M8; RVS CARROS.SLUITRING A2","M8; RVS CARROS.SLUITRING A2",null,"0,005 kg"]
[1,"467977CC","VERBINDINGSPLAAT STORTSCHOT CC.142","PLAAT 1740*162*3",null,"6,745 kg"]
[1,"537235CC","BEV.BUIS STORTSCHOT CC.142; BOVENBAND; R",null,null,"9,499 kg"]
[1,"537235CC_MIR","BEV.BUIS STORTSCHOT CC.142; BOVENBAND; L",null,null,"9,499 kg"]
[1,"537236CC","STORTSCHOT BOVENBAND; CC.142; L",null,null,"17,142 kg"]
[1,"537236CC_MIR","STORTSCHOT BOVENBAND; CC.142; R",null,null,"17,140 kg"]
[1,"517537CC","SCHRAPER INWENDIG CC.142",null,null,"15,029 kg"]
[13,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[13,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[26,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[1,"451226CC","SCHRAAPSTRIP L=1650","PLAT 100*10-1650",null,"1,072 kg"]
[2,"469328CC","KLEMPROFIEL SCHRAAPSTRIP","PLAAT 1650*109*4",null,"5,780 kg"]
[2,"538117CC","BEVESTIGINGSPROFIEL SCHRAPER",null,null,"1,016 kg"]
[10,"536725CC","TROGSTELBEUGEL CC.142; 30°; RVS","TROGSTELBEUGEL CC.142; 30°; RVS",null,"20,131 kg"]
[1,"536728CC","DRIJFTROMMEL 288*1500; BEKLEED",null,null,"151,435 kg"]
[1,"536734CC","TROGSTELBEUGEL CC.142; 15°; RVS",null,null,"18,811 kg"]
[2,"536741CC","VERBINDINGSBRUG ZIJPLATEN CC.142; 1730",null,null,"13,740 kg"]
[1,"537920CC","SPANNER DRIJFTROMMEL CC.142; SNL ø55; L",null,null,"21,519 kg"]
[1,"537920CC_MIR","SPANNER DRIJFTROMMEL CC.142; RECHTS",null,null,"21,519 kg"]
[2,"538045CC","BORGAS SCHRAPER INWENDIG",null,null,"0,632 kg"]
[1,"539104CC","ZIJKANT CC.142; KOPSTUK; 7205",null,null,"143,097 kg"]
[1,"539104CC_MIR","ZIJKANT CC.142; KOPSTUK; 720",null,null,"143,097 kg"]
[1,"518340CC","KOPSTUK BOVENBAND CC.142; R",null,null,"1109,088 kg"]
[2,"212009","M20; THVZ DRAADEIND; ISO; 8.8","M20; THVZ DRAADEIND; ISO; 8.8",null,"2,522 kg"]
[18,"217780","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART",null,"0,020 kg"]
[8,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[8,"221046","M10*20; ZK.TAPBOUT; RVS; A2","M10*20; ZK.TAPBOUT; RVS; A2",null,"0,025 kg"]
[66,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[3,"221073","M16*40; RVS ZK. TAPBOUT; A2 DIN933","M16*40; RVS ZK. TAPBOUT; A2 DIN933",null,"0,101 kg"]
[3,"221075","M16*50; ZK TAPBOUT; RVS; A2","M16*50; ZK TAPBOUT; RVS; A2",null,"0,116 kg"]
[4,"221243","M12*60; RVS ZK. BOUT; A2; DIN931","M12*60; RVS ZK. BOUT; A2; DIN931",null,"0,071 kg"]
[19,"221247","M12*90; RVS ZK. BOUT; A2","M12*90; RVS ZK. BOUT; A2",null,"0,095 kg"]
[8,"221253","M16*60; RVS ZK. BOUT; A2; DIN931","M16*60; RVS ZK. BOUT; A2; DIN931",null,"0,136 kg"]
[3,"221257","M16*80;ZK.RVS BOUT; A2","M16*80;ZK.RVS BOUT; A2",null,"0,163 kg"]
[22,"222244","M8*35;  A2;CIL.SCHR+BINNENZESK","M8*35;  A2;CIL.SCHR+BINNENZESK",null,"0,021 kg"]
[14,"223011","M20; ZK.MOER; RVS; A2","M20; ZK.MOER; RVS; A2",null,"0,065 kg"]
[30,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[71,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[15,"224462","M16; RVS BORGMOER; A2","M16; RVS BORGMOER; A2",null,"0,037 kg"]
[42,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[156,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[21,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[8,"225024","M10; CARROS.SLUITRING; RVS; A2","M10; CARROS.SLUITRING; RVS; A2",null,"0,012 kg"]
[12,"225026","M16; CARROS. SLUITRING","M16; CARROS. SLUITRING",null,"0,042 kg"]
[8,"225028","M20; RVS SLUITRING; A2; M20*44*8;DIN7349","M20; RVS SLUITRING; A2; M20*44*8;DIN7349",null,"0,075 kg"]
[20,"225057","M12; RVS VEERRING; A2; DIN127","M12; RVS VEERRING; A2; DIN127",null,"0,004 kg"]
[2,"225059","M16; RVS VEERRING; A2","M16; RVS VEERRING; A2",null,"0,008 kg"]
[2,"243279","22212 EK; TONLAGER; SKF","22212 EK; TONLAGER; SKF",null,"1,150 kg"]
[2,"243530","SNL 512-610; LAGERHUIS; SKF","SNL 512-610; LAGERHUIS; SKF",null,"5,740 kg"]
[1,"243602","ASNH 512-610 EINDDEKSEL; SKF","ASNH 512-610 EINDDEKSEL; SKF",null,"0,120 kg"]
["1,500 ul","243632","TSNA 512 A; AFDICHTING; SKF","TSNA 512 A; AFDICHTING; SKF",null,"0,060 kg"]
["4,000 ul","243694","FRB 10/110; AFSTANDSRING; SKF","FRB 10/110; AFSTANDSRING; SKF",null,"0,246 kg"]
[2,"243702","H 312; TREKBUS; SKF","H 312; TREKBUS; SKF",null,"0,400 kg"]
[4,"246405","ZIJGELEIDEROL ø63.5*100; B","ZIJGELEIDEROL ø63.5*100; B",null,"0,998 kg"]
[11,"246416","TRANSPORTROL ø89*530; AS ø20*560","TRANSPORTROL ø89*530; AS ø20*560",null,"4,000 kg"]
[4,"246435","TRANSPORTROL ø89*1550; AS ø25*1581","TRANSPORTROL ø89*1550; AS ø25*1581",null,"16,889 kg"]
[24,"246580","TRANSPORTROL ø89*465; AS ø20*495","TRANSPORTROL ø89*465; AS ø20*495",null,"3,500 kg"]
[2,"247562","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"1,203 kg"]
[1,"247562-1","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"0,470 kg"]
[2,"247562-2","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"0,366 kg"]
[1,"400586FS","SMEERBOUT M16*40","SMEERBOUT M16*40",null,"0,099 kg"]
[1,"211804","1/8\"G-180º; SMEERNIPPEL","1/8\"G-180º; SMEERNIPPEL",null,"0,008 kg"]
[1,"400586FS","TAPBOUT THVZ. M16*40","TAPBOUT THVZ. M16*40",null,"0,092 kg"]
[1,"400591RT","BORGSCHIJF KA76; ø70*ø17*8","BORGSCHIJF KA76; ø70*ø17*8",null,"0,079 kg"]
[1,"400128RT","BORGSCHIJF ø70*ø13*8;  KA76","PLAAT ø70*8",null,"0,081 kg"]
[19,"404008TS","AFSTANDSBUS TROGSTELBEUGEL TS","BUIS ø21,3*2,65-54",null,"0,067 kg"]
[1,"405035CC","OPVULBUS ø70*ø50-20","BUIS ø70*10-20",null,"0,291 kg"]
[2,"405065TF","AS ø6-1300","AS ø6-1300",null,"0,295 kg"]
[4,"405070TF","AS ø6-3000","AS ø6-3000",null,"0,681 kg"]
[1,"405210TS","OPVULBUS ø30*ø16,5*20,5","AS ø30-20,5",null,"0,081 kg"]
[2,"406253TS","DRAADSPIL M20*750; THVZ","DRAADSPIL M20*750; THVZ",null,"1,851 kg"]
[4,"406316CC","DRAADBUS TROGSTELBEUGEL BEGIN/EIND","AS ø20-54",null,"0,101 kg"]
[1,"448547CC","RUBBER SCHRAPER DR-TROMMEL CC/TS.140","PLAAT 1500*200*6",null,"1,790 kg"]
[1,"448548CC","KLEMSTRIP RUBBER; L=1480; HOH.200","PLAAT 1480*35*3",null,"1,234 kg"]
[2,"449350CC","BORGPLAAT STORTSCHOT CC.140","PLAAT 80*65*5",null,"0,085 kg"]
[1,"450871CC","SCHUIFBLOK REACTIEARM","PLAAT 115*30*12",null,"0,136 kg"]
[2,"451866CC","TREKSTRIP SCHOOR CC.160; L=2770","PLAAT 2810*40*5",null,"4,481 kg"]
[1,"467181CC","SCHRAPER KEERTROMMEL CC/TS.140","PLAAT 1600*264*4",null,"13,204 kg"]
[1,"467185CC","SCHRAPER DRIJFTROMMEL UITW; CC/TS.140","PLAAT 1743*116*5",null,"7,632 kg"]
[8,"467187CC","STEUNROLHOUDER CC.142","PLAAT 190*136*5",null,"0,868 kg"]
[2,"467210CC","STEUN GELEIDING STORTSCHOT CC.142","PLAAT 433*79*5",null,"0,859 kg"]
[4,"467212CC","BEV.BEUGEL ZIJGELEIDEROL CC.142","PLAAT 189*65*10",null,"0,904 kg"]
[2,"467217CC","BEV.STEUN TROGSTELBEUGEL STUREN CC.142","PLAAT 160*152*8",null,"1,177 kg"]
[1,"469048CC","BEV.STEUN SCHRAPER DRIJFTR CC.142; R","PLAAT 280*267*6",null,"1,397 kg"]
[1,"469048CC_MIR","BEV.STEUN SCHRAPER DRIJFTR CC.142; L","PLAAT 280*267*6",null,"1,397 kg"]
[1,"469070CC_MIR","REACTIEARM KA77","PLAAT 858*170*10",null,"6,913 kg"]
[1,"516338CC","TROGSTELBEUGEL CC.142; 10°; STUREN; KPL",null,null,"13,965 kg"]
[4,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[4,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[4,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[2,"467226CC","KLEMPLAAT DRAAGROL STUREN CC","PLAAT 148*60*5",null,"0,097 kg"]
[1,"536754CC","TROGSTELBEUGEL CC.142; 10°; STUREN",null,null,"13,664 kg"]
[1,"516606CC","STORTSCHOT BOVENBAND CC.142; KPL",null,null,"60,918 kg"]
[2,"218001","INSTEEKDOP ø42*1.3/3","INSTEEKDOP ø42*1.3/3",null,"0,009 kg"]
[8,"221035","M8*25; ZK.TAPBOUT; RVS, A2","M8*25; ZK.TAPBOUT; RVS, A2",null,"0,016 kg"]
[8,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[8,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[8,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[8,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[16,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[8,"225023","M8; RVS CARROS.SLUITRING A2","M8; RVS CARROS.SLUITRING A2",null,"0,005 kg"]
[1,"467977CC","VERBINDINGSPLAAT STORTSCHOT CC.142","PLAAT 1740*162*3",null,"6,745 kg"]
[1,"537235CC","BEV.BUIS STORTSCHOT CC.142; BOVENBAND; R",null,null,"9,499 kg"]
[1,"537235CC_MIR","BEV.BUIS STORTSCHOT CC.142; BOVENBAND; L",null,null,"9,499 kg"]
[1,"537236CC","STORTSCHOT BOVENBAND; CC.142; L",null,null,"17,142 kg"]
[1,"537236CC_MIR","STORTSCHOT BOVENBAND; CC.142; R",null,null,"17,140 kg"]
[1,"517537CC","SCHRAPER INWENDIG CC.142",null,null,"15,029 kg"]
[13,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[13,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[26,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[1,"451226CC","SCHRAAPSTRIP L=1650","PLAT 100*10-1650",null,"1,072 kg"]
[2,"469328CC","KLEMPROFIEL SCHRAAPSTRIP","PLAAT 1650*109*4",null,"5,780 kg"]
[2,"538117CC","BEVESTIGINGSPROFIEL SCHRAPER",null,null,"1,016 kg"]
[10,"536725CC","TROGSTELBEUGEL CC.142; 30°; RVS","TROGSTELBEUGEL CC.142; 30°; RVS",null,"20,131 kg"]
[1,"536728CC","DRIJFTROMMEL 288*1500; BEKLEED",null,null,"151,435 kg"]
[1,"536734CC","TROGSTELBEUGEL CC.142; 15°; RVS",null,null,"18,811 kg"]
[1,"536741CC","VERBINDINGSBRUG ZIJPLATEN CC.142; 1730",null,null,"13,740 kg"]
[1,"537920CC","SPANNER DRIJFTROMMEL CC.142; SNL ø55; L",null,null,"21,519 kg"]
[1,"537920CC_MIR","SPANNER DRIJFTROMMEL CC.142; RECHTS",null,null,"21,519 kg"]
[2,"538045CC","BORGAS SCHRAPER INWENDIG",null,null,"0,632 kg"]
[1,"539104CC","ZIJKANT CC.142; KOPSTUK; 7205",null,null,"143,097 kg"]
[1,"539104CC_MIR","ZIJKANT CC.142; KOPSTUK; 720",null,null,"143,097 kg"]
[1,"518687CC","TUSSENSTUK  BOVENBAND CC.142; 5950","TUSSENSTUK  BOVENBAND CC.142; 5950",null,"611,412 kg"]
[18,"217780","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART",null,"0,020 kg"]
[4,"221046","M10*20; ZK.TAPBOUT; RVS; A2","M10*20; ZK.TAPBOUT; RVS; A2",null,"0,025 kg"]
[28,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[2,"221073","M16*40; RVS ZK. TAPBOUT; A2 DIN933","M16*40; RVS ZK. TAPBOUT; A2 DIN933",null,"0,101 kg"]
[4,"221075","M16*50; ZK TAPBOUT; RVS; A2","M16*50; ZK TAPBOUT; RVS; A2",null,"0,116 kg"]
[16,"221247","M12*90; RVS ZK. BOUT; A2","M12*90; RVS ZK. BOUT; A2",null,"0,095 kg"]
[4,"221253","M16*60; RVS ZK. BOUT; A2; DIN931","M16*60; RVS ZK. BOUT; A2; DIN931",null,"0,136 kg"]
[18,"222244","M8*35;  A2;CIL.SCHR+BINNENZESK","M8*35;  A2;CIL.SCHR+BINNENZESK",null,"0,021 kg"]
[18,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[46,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[10,"224462","M16; RVS BORGMOER; A2","M16; RVS BORGMOER; A2",null,"0,037 kg"]
[18,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[90,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[14,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[4,"225024","M10; CARROS.SLUITRING; RVS; A2","M10; CARROS.SLUITRING; RVS; A2",null,"0,012 kg"]
[8,"225026","M16; CARROS. SLUITRING","M16; CARROS. SLUITRING",null,"0,042 kg"]
[2,"246405","ZIJGELEIDEROL ø63.5*100; B","ZIJGELEIDEROL ø63.5*100; B",null,"0,998 kg"]
[9,"246416","TRANSPORTROL ø89*530; AS ø20*560","TRANSPORTROL ø89*530; AS ø20*560",null,"4,000 kg"]
[4,"246435","TRANSPORTROL ø89*1550; AS ø25*1581","TRANSPORTROL ø89*1550; AS ø25*1581",null,"16,889 kg"]
[18,"246580","TRANSPORTROL ø89*465; AS ø20*495","TRANSPORTROL ø89*465; AS ø20*495",null,"3,500 kg"]
[2,"247562","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"1,203 kg"]
[1,"247562-1","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"0,470 kg"]
[2,"247562-2","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"0,366 kg"]
[16,"404008TS","AFSTANDSBUS TROGSTELBEUGEL TS","BUIS ø21,3*2,65-54",null,"0,067 kg"]
[4,"405070TF","AS ø6-3000","AS ø6-3000",null,"0,681 kg"]
[2,"453876CC","TREKSTRIP SCHOOR CC.142; L=2960","PLAAT 3000*40*5",null,"4,786 kg"]
[8,"467187CC","STEUNROLHOUDER CC.142","PLAAT 190*136*5",null,"0,868 kg"]
[2,"467212CC","BEV.BEUGEL ZIJGELEIDEROL CC.142","PLAAT 189*65*10",null,"0,904 kg"]
[9,"536725CC","TROGSTELBEUGEL CC.142; 30°; RVS","TROGSTELBEUGEL CC.142; 30°; RVS",null,"20,131 kg"]
[1,"536741CC","VERBINDINGSBRUG ZIJPLATEN CC.142; 1730",null,null,"13,740 kg"]
[2,"539434CC","ZIJKANT CC.142; MIDDEN; 5950","ZIJKANT CC.142; MIDDEN; 5950",null,"107,991 kg"]
[1,"539136CC","MEENEMER VLAKKABEL CC.142; BOVENBAND",null,null,"1,887 kg"]
[1,"539147CC","STEUN E-KAST BOVENBAND CC.142; RECHTS",null,null,"2,649 kg"]
[1,"539147CC_MIR","STEUN E-KAST BOVENBAND CC.142; LINKS",null,null,"2,649 kg"]
[1,"518680CC","OPHANGING CC.142-501420CC",null,null,"3264,260 kg"]
[16,"221048","M10*30; ZK.TAPBOUT; RVS; A2","M10*30; ZK.TAPBOUT; RVS; A2",null,"0,032 kg"]
[64,"221050","M10*40; ZK.TAPBOUT; RVS; A2","M10*40; ZK.TAPBOUT; RVS; A2",null,"0,038 kg"]
[20,"221075","M16*50; ZK TAPBOUT; RVS; A2","M16*50; ZK TAPBOUT; RVS; A2",null,"0,116 kg"]
[64,"223006","M10; ZK.MOER; RVS; A2","M10; ZK.MOER; RVS; A2",null,"0,011 kg"]
[20,"223009","M16; ZK.MOER; RVS; A2","M16; ZK.MOER; RVS; A2",null,"0,034 kg"]
[16,"224459","M10; RVS BORGMOER; A2; DIN 985","M10; RVS BORGMOER; A2; DIN 985",null,"0,014 kg"]
[128,"225006","M10; RVS SLUITRING; A2; DIN125A","M10; RVS SLUITRING; A2; DIN125A",null,"0,004 kg"]
[20,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[32,"225024","M10; CARROS.SLUITRING; RVS; A2","M10; CARROS.SLUITRING; RVS; A2",null,"0,012 kg"]
[20,"225026","M16; CARROS. SLUITRING","M16; CARROS. SLUITRING",null,"0,042 kg"]
[40,"452896CC","OPVULPLAAT OPHANGRAILS CC.162; S=2","PLAAT 150*110*2",null,"0,247 kg"]
[2,"453329CC","DRAAGBALK VLAKKABELRAIL; L=4340","IPE100-4340",null,"35,195 kg"]
[6,"453874CC","OPVULPLAAT VERBINDINGSBUIS","PLAAT 240*200*3",null,"0,902 kg"]
[8,"517330CC","OPHANGRAILS CC.142; 4460; LINKS",null,null,"152,025 kg"]
[13,"221047","M10*25; ZK.TAPBOUT; RVS; A2","M10*25; ZK.TAPBOUT; RVS; A2",null,"0,029 kg"]
[8,"221048","M10*30; ZK.TAPBOUT; RVS; A2","M10*30; ZK.TAPBOUT; RVS; A2",null,"0,032 kg"]
[8,"221075","M16*50; ZK TAPBOUT; RVS; A2","M16*50; ZK TAPBOUT; RVS; A2",null,"0,116 kg"]
[21,"224459","M10; RVS BORGMOER; A2; DIN 985","M10; RVS BORGMOER; A2; DIN 985",null,"0,014 kg"]
[8,"224462","M16; RVS BORGMOER; A2","M16; RVS BORGMOER; A2",null,"0,037 kg"]
[16,"225006","M10; RVS SLUITRING; A2; DIN125A","M10; RVS SLUITRING; A2; DIN125A",null,"0,004 kg"]
[16,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[2,"448926CC","KOPPELPLAAT OPHANGRAILS CC","PLAAT 320*120*8",null,"2,407 kg"]
[2,"469050CC","U-PROFIEL OPHANGRAILS CC.142; 4459; L","PLAAT 4459*407*5",null,"72,411 kg"]
[8,"517331CC","OPHANGRAILS CC.142; 4460; RECHTS",null,null,"149,587 kg"]
[13,"221047","M10*25; ZK.TAPBOUT; RVS; A2","M10*25; ZK.TAPBOUT; RVS; A2",null,"0,029 kg"]
[8,"221048","M10*30; ZK.TAPBOUT; RVS; A2","M10*30; ZK.TAPBOUT; RVS; A2",null,"0,032 kg"]
[8,"221075","M16*50; ZK TAPBOUT; RVS; A2","M16*50; ZK TAPBOUT; RVS; A2",null,"0,116 kg"]
[21,"224459","M10; RVS BORGMOER; A2; DIN 985","M10; RVS BORGMOER; A2; DIN 985",null,"0,014 kg"]
[8,"224462","M16; RVS BORGMOER; A2","M16; RVS BORGMOER; A2",null,"0,037 kg"]
[16,"225006","M10; RVS SLUITRING; A2; DIN125A","M10; RVS SLUITRING; A2; DIN125A",null,"0,004 kg"]
[16,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[2,"448926CC","KOPPELPLAAT OPHANGRAILS CC","PLAAT 320*120*8",null,"2,407 kg"]
[2,"469051CC","U-PROFIEL OPHANGRAILS CC.142; 4459; R","PLAAT 4459*407*5",null,"71,192 kg"]
[1,"518684CC","OPHANGRAILS CC.142; 4460; EIND; LINKS",null,null,"27,452 kg"]
[13,"221047","M10*25; ZK.TAPBOUT; RVS; A2","M10*25; ZK.TAPBOUT; RVS; A2",null,"0,029 kg"]
[8,"221048","M10*30; ZK.TAPBOUT; RVS; A2","M10*30; ZK.TAPBOUT; RVS; A2",null,"0,032 kg"]
[8,"221075","M16*50; ZK TAPBOUT; RVS; A2","M16*50; ZK TAPBOUT; RVS; A2",null,"0,116 kg"]
[21,"224459","M10; RVS BORGMOER; A2; DIN 985","M10; RVS BORGMOER; A2; DIN 985",null,"0,014 kg"]
[8,"224462","M16; RVS BORGMOER; A2","M16; RVS BORGMOER; A2",null,"0,037 kg"]
[16,"225006","M10; RVS SLUITRING; A2; DIN125A","M10; RVS SLUITRING; A2; DIN125A",null,"0,004 kg"]
[16,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[3,"448926CC","KOPPELPLAAT OPHANGRAILS CC","PLAAT 320*120*8",null,"2,407 kg"]
[1,"470808CC","U-PROFIEL OPHANGRAILS CC.142; 4460; L","PLAAT 4459*407*5",null,"8,921 kg"]
[1,"470808CC_MIR","U-PROFIEL OPHANGRAILS CC.142; 4460; R","PLAAT 4459*407*5",null,"8,921 kg"]
[1,"518685CC","OPHANGRAILS CC.142; 4460; RECHTS","OPHANGRAILS CC.142; 4460; RECHTS",null,"151,463 kg"]
[13,"221047","M10*25; ZK.TAPBOUT; RVS; A2","M10*25; ZK.TAPBOUT; RVS; A2",null,"0,029 kg"]
[8,"221048","M10*30; ZK.TAPBOUT; RVS; A2","M10*30; ZK.TAPBOUT; RVS; A2",null,"0,032 kg"]
[8,"221075","M16*50; ZK TAPBOUT; RVS; A2","M16*50; ZK TAPBOUT; RVS; A2",null,"0,116 kg"]
[21,"224459","M10; RVS BORGMOER; A2; DIN 985","M10; RVS BORGMOER; A2; DIN 985",null,"0,014 kg"]
[8,"224462","M16; RVS BORGMOER; A2","M16; RVS BORGMOER; A2",null,"0,037 kg"]
[16,"225006","M10; RVS SLUITRING; A2; DIN125A","M10; RVS SLUITRING; A2; DIN125A",null,"0,004 kg"]
[16,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[3,"448926CC","KOPPELPLAAT OPHANGRAILS CC","PLAAT 320*120*8",null,"2,407 kg"]
[2,"470809CC ","U-PROFIEL OPHANGRAILS CC.142; 4460; R","PLAAT 4459*407*5",null,"70,927 kg"]
[2,"518686CC","OPHANGRAILS CC.142; 4500/5980; LINKS; EIND",null,null,"198,704 kg"]
[29,"221048","M10*30; ZK.TAPBOUT; RVS; A2","M10*30; ZK.TAPBOUT; RVS; A2",null,"0,032 kg"]
[10,"221075","M16*50; ZK TAPBOUT; RVS; A2","M16*50; ZK TAPBOUT; RVS; A2",null,"0,116 kg"]
[6,"221076","M16*60; RVS ZK. TAPBOUT; A2","M16*60; RVS ZK. TAPBOUT; A2",null,"0,132 kg"]
[29,"224459","M10; RVS BORGMOER; A2; DIN 985","M10; RVS BORGMOER; A2; DIN 985",null,"0,014 kg"]
[16,"224462","M16; RVS BORGMOER; A2","M16; RVS BORGMOER; A2",null,"0,037 kg"]
[58,"225006","M10; RVS SLUITRING; A2; DIN125A","M10; RVS SLUITRING; A2; DIN125A",null,"0,004 kg"]
[32,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[1,"453402CC","KOPPELPLAAT OPHANGRAILS CC","PLAAT 210*120*5",null,"0,988 kg"]
[1,"470611CC","KOPPELPLAAT OPHANGRAILS CC","PLAAT 450*229*8",null,"4,925 kg"]
[1,"470810CC","U-PROFIEL OPHANGRAILS CC.142; 5980; L; EIND","PLAAT 5979*407*5",null,"94,171 kg"]
[1,"470810CC_MIR","U-PROFIEL OPHANGRAILS CC.142; 5980; R; EIND","PLAAT 5979*407*5",null,"94,171 kg"]
[2,"536929CC","EINDAANSLAG CC.142; ONDERBAND",null,null,"4,465 kg"]
[1,"537929CC","EINDAANSLAG CC.142; BOVENBAND",null,null,"6,643 kg"]
[1,"537929CC_MIR","EINDAANSLAG CC.142; BOVENBAND; RECHTS",null,null,"6,643 kg"]
[1,"539197CC","VERBINDINGSBUIS; 3868",null,null,"54,013 kg"]
[1,"539198CC","VERBINDINGSBUIS; 2770",null,null,"52,278 kg"]
[10,"539277CC","OPHANGBEUGEL IPE100; VLAKKABELRAIL",null,null,"8,185 kg"]
[2,"539433CC","SCHOORBUIS H.O.H.2950; ",null,null,"65,190 kg"]
[1,"518681CC","ONDERBAND CC.142-501420CC",null,null,"4043,606 kg"]
[1,null,"E-KAST 500x500x210 (CONTROLS)","E-KAST 500x500x210 (CONTROLS)",null,"15,591 kg"]
[4,"221040","M8*50; RVS ZK.TAPBOUT; A2","M8*50; RVS ZK.TAPBOUT; A2",null,"0,003 kg"]
[4,"223005","M8; ZK.MOER; RVS; A2","M8; ZK.MOER; RVS; A2",null,"0,005 kg"]
[1,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[1,"E-KAST RITTAL AE 1007.600 (500-500-210)","RITTAL AE 1007.600 (500*500*210)","RITTAL AE 1007.600 (500*500*210)",null,"15,555 kg"]
[8,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[4,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[10,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[4,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[18,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[2,"262213-M3-270gr-3","KA77 DRN132M4; 7,5; N=99; 480; 60; M3A","KA77 DRN132M4; 7,5; N=99; 480; 60; M3A",null,"126,000 kg"]
[2,"262344-M1-0gr-X","RF07 DRN71MS4; 0.25; N=51; 480; M1","RF07 DRN71MS4; 0.25; N=51; 480; M1",null,"9,300 kg"]
[2,"262350-M1-0gr-X","RF07 DRN71MS4/BE03HR","RF07 DRN71MS4/BE03HR",null,"37,000 kg"]
[2,"262924","BUFFER MET DRAADEIND; DEMAG 233.701.045","BUFFER MET DRAADEIND; DEMAG 233.701.045",null,"0,236 kg"]
[1,"470447CC","BEV.STEUN E-KAST CC.142; LINKS","PLAAT 680*202*3",null,"2,259 kg"]
[1,"470447CC_MIR","BEV.STEUN E-KAST CC.142; RECHTS","PLAAT 680*202*3",null,"2,259 kg"]
[1,"480452CC","TR-BAND; RUB; 1400*43000","TR-BAND; RUB; 1400*43000",null,"601,491 kg"]
[6,"516335CC","LOOPWAGEN ONDERBAND CC.142; VRIJLOOP",null,null,"21,222 kg"]
[5,"224464","M20; RVS BORGMOER; A2","M20; RVS BORGMOER; A2",null,"0,072 kg"]
[6,"225011","M20; RVS SLUITRING; A2; DIN125A","M20; RVS SLUITRING; A2; DIN125A",null,"0,018 kg"]
[2,"405041CC","TUSSENAS LOOPWAGEN ONDERBAND CC; L=226","AS ø30-226",null,"1,094 kg"]
[1,"405042CC","SCHARNIERBUIS LOOPWAGEN CC; L=180","BUIS ø26,9*2,65-180",null,"0,292 kg"]
[2,"405043CC","OPVULBUS OPHANGSTEUN CC.142; L=20","BUIS ø33,7*2,6-20",null,"0,041 kg"]
[2,"446001CC","ZIJPLAAT LOOPWAGEN SCHUIFBAND","PLAAT 286*250*10",null,"4,511 kg"]
[4,"515508CC","LOOPROL SCHUIFBAND VRIJLOOP; KPL",null,null,"2,140 kg"]
[1,"221085","M20*50; ZK.RVS.TAPBOUT; A2","M20*50; ZK.RVS.TAPBOUT; A2",null,"0,199 kg"]
[1,"225011","M20; RVS SLUITRING; A2; DIN125A","M20; RVS SLUITRING; A2; DIN125A",null,"0,018 kg"]
[1,"225061","M20; VEERRING; RVS; A2","M20; VEERRING; RVS; A2",null,"0,013 kg"]
[1,"225425","ASBORGRING ø35; RVS","ASBORGRING ø35; RVS",null,"0,004 kg"]
[1,"225558","GATBORGRING; G72; RVS","GATBORGRING; G72; RVS",null,"0,020 kg"]
[1,"243060","KOGELLAGER 6207-2RS1; RVS KOGELLAGER","KOGELLAGER 6207-2RS1; RVS KOGELLAGER",null,"0,281 kg"]
[1,"404048CC","AS LOOPROL SCHUIFBAND","AS ø40-43",null,"0,299 kg"]
[1,"535595CC","LOOPROL SCHUIFBAND VRIJLOOP",null,null,"1,305 kg"]
[1,"536747CC","SCHARNIERBOUT M20*206",null,null,"0,615 kg"]
[4,"516336CC","LOOPWAGEN ONDERBAND CC.142; AANDR",null,null,"21,156 kg"]
[4,"221025","M6*30; ZK.TAPBOUT; RVS; A2","M6*30; ZK.TAPBOUT; RVS; A2",null,"0,009 kg"]
[4,"224457","M6; RVS BORGMOER; A2","M6; RVS BORGMOER; A2",null,"0,003 kg"]
[5,"224464","M20; RVS BORGMOER; A2","M20; RVS BORGMOER; A2",null,"0,072 kg"]
[4,"225004","M6; RVS SLUITRING; A2; DIN125A","M6; RVS SLUITRING; A2; DIN125A",null,"0,001 kg"]
[6,"225011","M20; RVS SLUITRING; A2; DIN125A","M20; RVS SLUITRING; A2; DIN125A",null,"0,018 kg"]
[1,"404055CC","TANDWIEL AANDRIJVING RIJWERK SCHUIFBAND",null,null,"0,321 kg"]
[1,"245811","TANDWIEL; Z=15; M=3; RVS","TANDWIEL; Z=15; M=3; RVS",null,"0,402 kg"]
[2,"405041CC","TUSSENAS LOOPWAGEN ONDERBAND CC; L=226","AS ø30-226",null,"1,094 kg"]
[1,"405042CC","SCHARNIERBUIS LOOPWAGEN CC; L=180","BUIS ø26,9*2,65-180",null,"0,292 kg"]
[2,"405043CC","OPVULBUS OPHANGSTEUN CC.142; L=20","BUIS ø33,7*2,6-20",null,"0,041 kg"]
[1,"446001CC","ZIJPLAAT LOOPWAGEN SCHUIFBAND","PLAAT 286*250*10",null,"4,511 kg"]
[1,"446155CC","ZIJPLAAT LOOPWAGEN SCHUIFBAND","PLAAT 286*250*10",null,"4,085 kg"]
[2,"515507CC","LOOPROL SCHUIFBAND AANGEDREVEN; KPL",null,null,"2,132 kg"]
[1,"221085","M20*50; ZK.RVS.TAPBOUT; A2","M20*50; ZK.RVS.TAPBOUT; A2",null,"0,199 kg"]
[1,"225011","M20; RVS SLUITRING; A2; DIN125A","M20; RVS SLUITRING; A2; DIN125A",null,"0,018 kg"]
[1,"225061","M20; VEERRING; RVS; A2","M20; VEERRING; RVS; A2",null,"0,013 kg"]
[1,"225425","ASBORGRING ø35; RVS","ASBORGRING ø35; RVS",null,"0,004 kg"]
[1,"225558","GATBORGRING; G72; RVS","GATBORGRING; G72; RVS",null,"0,020 kg"]
[1,"243060","KOGELLAGER 6207-2RS1; RVS KOGELLAGER","KOGELLAGER 6207-2RS1; RVS KOGELLAGER",null,"0,281 kg"]
[1,"404048CC","AS LOOPROL SCHUIFBAND","AS ø40-43",null,"0,299 kg"]
[1,"535594CC","LOOPROL SCHUIFBAND AANGEDREVEN",null,null,"1,298 kg"]
[2,"515508CC","LOOPROL SCHUIFBAND VRIJLOOP; KPL",null,null,"2,140 kg"]
[1,"221085","M20*50; ZK.RVS.TAPBOUT; A2","M20*50; ZK.RVS.TAPBOUT; A2",null,"0,199 kg"]
[1,"225011","M20; RVS SLUITRING; A2; DIN125A","M20; RVS SLUITRING; A2; DIN125A",null,"0,018 kg"]
[1,"225061","M20; VEERRING; RVS; A2","M20; VEERRING; RVS; A2",null,"0,013 kg"]
[1,"225425","ASBORGRING ø35; RVS","ASBORGRING ø35; RVS",null,"0,004 kg"]
[1,"225558","GATBORGRING; G72; RVS","GATBORGRING; G72; RVS",null,"0,020 kg"]
[1,"243060","KOGELLAGER 6207-2RS1; RVS KOGELLAGER","KOGELLAGER 6207-2RS1; RVS KOGELLAGER",null,"0,281 kg"]
[1,"404048CC","AS LOOPROL SCHUIFBAND","AS ø40-43",null,"0,299 kg"]
[1,"535595CC","LOOPROL SCHUIFBAND VRIJLOOP",null,null,"1,305 kg"]
[1,"536747CC","SCHARNIERBOUT M20*206",null,null,"0,615 kg"]
[2,"518413CC","TUSSENSTUK  ONDERBAND CC.142; 4380",null,null,"421,458 kg"]
[10,"217780","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART",null,"0,020 kg"]
[4,"221046","M10*20; ZK.TAPBOUT; RVS; A2","M10*20; ZK.TAPBOUT; RVS; A2",null,"0,025 kg"]
[18,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[8,"221072","M16*35; ZK. RVS TAPBOUT; A2","M16*35; ZK. RVS TAPBOUT; A2",null,"0,093 kg"]
[2,"221073","M16*40; RVS ZK. TAPBOUT; A2 DIN933","M16*40; RVS ZK. TAPBOUT; A2 DIN933",null,"0,101 kg"]
[4,"221075","M16*50; ZK TAPBOUT; RVS; A2","M16*50; ZK TAPBOUT; RVS; A2",null,"0,116 kg"]
[12,"221247","M12*90; RVS ZK. BOUT; A2","M12*90; RVS ZK. BOUT; A2",null,"0,095 kg"]
[10,"222244","M8*35;  A2;CIL.SCHR+BINNENZESK","M8*35;  A2;CIL.SCHR+BINNENZESK",null,"0,021 kg"]
[10,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[30,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[14,"224462","M16; RVS BORGMOER; A2","M16; RVS BORGMOER; A2",null,"0,037 kg"]
[10,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[60,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[26,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[4,"225024","M10; CARROS.SLUITRING; RVS; A2","M10; CARROS.SLUITRING; RVS; A2",null,"0,012 kg"]
[4,"225026","M16; CARROS. SLUITRING","M16; CARROS. SLUITRING",null,"0,042 kg"]
[2,"246405","ZIJGELEIDEROL ø63.5*100; B","ZIJGELEIDEROL ø63.5*100; B",null,"0,998 kg"]
[6,"246416","TRANSPORTROL ø89*530; AS ø20*560","TRANSPORTROL ø89*530; AS ø20*560",null,"4,000 kg"]
[2,"246435","TRANSPORTROL ø89*1550; AS ø25*1581","TRANSPORTROL ø89*1550; AS ø25*1581",null,"16,889 kg"]
[12,"246580","TRANSPORTROL ø89*465; AS ø20*495","TRANSPORTROL ø89*465; AS ø20*495",null,"3,500 kg"]
[2,"247562","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"1,203 kg"]
[1,"247562-1","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"0,470 kg"]
[2,"247562-2","SPANSCHROEF 2*OOG; M16; RVS","SPANSCHROEF 2*OOG; M16; RVS",null,"0,366 kg"]
[12,"404008TS","AFSTANDSBUS TROGSTELBEUGEL TS","BUIS ø21,3*2,65-54",null,"0,067 kg"]
[4,"405070TF","AS ø6-3000","AS ø6-3000",null,"0,681 kg"]
[2,"451866CC","TREKSTRIP SCHOOR CC.160; L=2770","PLAAT 2810*40*5",null,"4,481 kg"]
[4,"467187CC","STEUNROLHOUDER CC.142","PLAAT 190*136*5",null,"0,868 kg"]
[2,"467212CC","BEV.BEUGEL ZIJGELEIDEROL CC.142","PLAAT 189*65*10",null,"0,904 kg"]
[6,"536725CC","TROGSTELBEUGEL CC.142; 30°; RVS","TROGSTELBEUGEL CC.142; 30°; RVS",null,"20,131 kg"]
[2,"448524CC",null,"PLAAT 320*50*5",null,"0,642 kg"]
[1,"467176CC",null,"PLAAT 1730*219*5",null,"15,163 kg"]
[2,"467177CC",null,"PLAAT 361*60*8",null,"1,289 kg"]
[2,"467197CC",null,"PLAAT 253*60*5",null,"0,553 kg"]
[1,"536741CC","VERBINDINGSBRUG ZIJPLATEN CC.142; 1730",null,null,"13,740 kg"]
[2,"539207CC","ZIJKANT CC.142; MIDDEN; 4380",null,null,"79,493 kg"]
[1,"518415CC","EINDSTUKL ONDERBAND CC.142; L",null,null,"976,450 kg"]
[2,"212009","M20; THVZ DRAADEIND; ISO; 8.8","M20; THVZ DRAADEIND; ISO; 8.8",null,"2,522 kg"]
[14,"217780","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART",null,"0,020 kg"]
[8,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[6,"221046","M10*20; ZK.TAPBOUT; RVS; A2","M10*20; ZK.TAPBOUT; RVS; A2",null,"0,025 kg"]
[70,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[2,"221063","M12*50; RVS ZK. TAPBOUT; A2","M12*50; RVS ZK. TAPBOUT; A2",null,"0,060 kg"]
[12,"221072","M16*35; ZK. RVS TAPBOUT; A2","M16*35; ZK. RVS TAPBOUT; A2",null,"0,093 kg"]
[4,"221243","M12*60; RVS ZK. BOUT; A2; DIN931","M12*60; RVS ZK. BOUT; A2; DIN931",null,"0,071 kg"]
[14,"221247","M12*90; RVS ZK. BOUT; A2","M12*90; RVS ZK. BOUT; A2",null,"0,095 kg"]
[2,"221253","M16*60; RVS ZK. BOUT; A2; DIN931","M16*60; RVS ZK. BOUT; A2; DIN931",null,"0,136 kg"]
[3,"221257","M16*80;ZK.RVS BOUT; A2","M16*80;ZK.RVS BOUT; A2",null,"0,163 kg"]
[18,"222244","M8*35;  A2;CIL.SCHR+BINNENZESK","M8*35;  A2;CIL.SCHR+BINNENZESK",null,"0,021 kg"]
[14,"223011","M20; ZK.MOER; RVS; A2","M20; ZK.MOER; RVS; A2",null,"0,065 kg"]
[26,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[72,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[15,"224462","M16; RVS BORGMOER; A2","M16; RVS BORGMOER; A2",null,"0,037 kg"]
[38,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[158,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[31,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[6,"225024","M10; CARROS.SLUITRING; RVS; A2","M10; CARROS.SLUITRING; RVS; A2",null,"0,012 kg"]
[2,"225026","M16; CARROS. SLUITRING","M16; CARROS. SLUITRING",null,"0,042 kg"]
[8,"225028","M20; RVS SLUITRING; A2; M20*44*8;DIN7349","M20; RVS SLUITRING; A2; M20*44*8;DIN7349",null,"0,075 kg"]
[20,"225057","M12; RVS VEERRING; A2; DIN127","M12; RVS VEERRING; A2; DIN127",null,"0,004 kg"]
[2,"225059","M16; RVS VEERRING; A2","M16; RVS VEERRING; A2",null,"0,008 kg"]
[2,"243279","22212 EK; TONLAGER; SKF","22212 EK; TONLAGER; SKF",null,"1,150 kg"]
[2,"243530","SNL 512-610; LAGERHUIS; SKF","SNL 512-610; LAGERHUIS; SKF",null,"5,740 kg"]
[1,"243602","ASNH 512-610 EINDDEKSEL; SKF","ASNH 512-610 EINDDEKSEL; SKF",null,"0,120 kg"]
["1,500 ul","243632","TSNA 512 A; AFDICHTING; SKF","TSNA 512 A; AFDICHTING; SKF",null,"0,060 kg"]
["4,000 ul","243694","FRB 10/110; AFSTANDSRING; SKF","FRB 10/110; AFSTANDSRING; SKF",null,"0,246 kg"]
[2,"243702","H 312; TREKBUS; SKF","H 312; TREKBUS; SKF",null,"0,400 kg"]
[2,"246405","ZIJGELEIDEROL ø63.5*100; B","ZIJGELEIDEROL ø63.5*100; B",null,"0,998 kg"]
[9,"246416","TRANSPORTROL ø89*530; AS ø20*560","TRANSPORTROL ø89*530; AS ø20*560",null,"4,000 kg"]
[3,"246435","TRANSPORTROL ø89*1550; AS ø25*1581","TRANSPORTROL ø89*1550; AS ø25*1581",null,"16,889 kg"]
[20,"246580","TRANSPORTROL ø89*465; AS ø20*495","TRANSPORTROL ø89*465; AS ø20*495",null,"3,500 kg"]
[1,"400586FS","SMEERBOUT M16*40","SMEERBOUT M16*40",null,"0,099 kg"]
[1,"211804","1/8\"G-180º; SMEERNIPPEL","1/8\"G-180º; SMEERNIPPEL",null,"0,008 kg"]
[1,"400586FS","TAPBOUT THVZ. M16*40","TAPBOUT THVZ. M16*40",null,"0,092 kg"]
[1,"400591RT","BORGSCHIJF KA76; ø70*ø17*8","BORGSCHIJF KA76; ø70*ø17*8",null,"0,079 kg"]
[1,"400128RT","BORGSCHIJF ø70*ø13*8;  KA76","PLAAT ø70*8",null,"0,081 kg"]
[14,"404008TS","AFSTANDSBUS TROGSTELBEUGEL TS","BUIS ø21,3*2,65-54",null,"0,067 kg"]
[1,"405035CC","OPVULBUS ø70*ø50-20","BUIS ø70*10-20",null,"0,291 kg"]
[4,"405070TF","AS ø6-3000","AS ø6-3000",null,"0,681 kg"]
[1,"405210TS","OPVULBUS ø30*ø16,5*20,5","AS ø30-20,5",null,"0,081 kg"]
[2,"406253TS","DRAADSPIL M20*750; THVZ","DRAADSPIL M20*750; THVZ",null,"1,851 kg"]
[4,"406316CC","DRAADBUS TROGSTELBEUGEL BEGIN/EIND","AS ø20-54",null,"0,101 kg"]
[1,"448548CC","KLEMSTRIP RUBBER; L=1480; HOH.200","PLAAT 1480*35*3",null,"1,234 kg"]
[1,"449184CC","RUBBER SCHRAPER DR-TR CC.142; 1500*400","PLAAT 1500*400*6",null,"3,596 kg"]
[2,"449350CC","BORGPLAAT STORTSCHOT CC.140","PLAAT 80*65*5",null,"0,085 kg"]
[1,"450871CC","SCHUIFBLOK REACTIEARM","PLAAT 115*30*12",null,"0,136 kg"]
[1,"467181CC","SCHRAPER KEERTROMMEL CC/TS.140","PLAAT 1600*264*4",null,"13,204 kg"]
[1,"467185CC","SCHRAPER DRIJFTROMMEL UITW; CC/TS.140","PLAAT 1743*116*5",null,"7,632 kg"]
[6,"467187CC","STEUNROLHOUDER CC.142","PLAAT 190*136*5",null,"0,868 kg"]
[2,"467210CC","STEUN GELEIDING STORTSCHOT CC.142","PLAAT 433*79*5",null,"0,859 kg"]
[2,"467212CC","BEV.BEUGEL ZIJGELEIDEROL CC.142","PLAAT 189*65*10",null,"0,904 kg"]
[2,"467217CC","BEV.STEUN TROGSTELBEUGEL STUREN CC.142","PLAAT 160*152*8",null,"1,177 kg"]
[1,"467876CC","ONDERSTEUNINGSPROFIEL RUBBER SCHRAPER CC.142","PLAAT 1490*181*3",null,"6,472 kg"]
[1,"469048CC","BEV.STEUN SCHRAPER DRIJFTR CC.142; R","PLAAT 280*267*6",null,"1,397 kg"]
[1,"469048CC_MIR","BEV.STEUN SCHRAPER DRIJFTR CC.142; L","PLAAT 280*267*6",null,"1,397 kg"]
[1,"469070CC","REACTIEARM KA77","PLAAT 858*170*10",null,"6,913 kg"]
[1,"516338CC","TROGSTELBEUGEL CC.142; 10°; STUREN; KPL",null,null,"13,965 kg"]
[4,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[4,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[4,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[2,"467226CC","KLEMPLAAT DRAAGROL STUREN CC","PLAAT 148*60*5",null,"0,097 kg"]
[1,"536754CC","TROGSTELBEUGEL CC.142; 10°; STUREN",null,null,"13,664 kg"]
[1,"517537CC","SCHRAPER INWENDIG CC.142",null,null,"15,029 kg"]
[13,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[13,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[26,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[1,"451226CC","SCHRAAPSTRIP L=1650","PLAT 100*10-1650",null,"1,072 kg"]
[2,"469328CC","KLEMPROFIEL SCHRAAPSTRIP","PLAAT 1650*109*4",null,"5,780 kg"]
[2,"538117CC","BEVESTIGINGSPROFIEL SCHRAPER",null,null,"1,016 kg"]
[1,"518330CC","STORTKLEP ONDERBAND CC.142; KPL",null,null,"55,681 kg"]
[2,"218001","INSTEEKDOP ø42*1.3/3","INSTEEKDOP ø42*1.3/3",null,"0,009 kg"]
[8,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[2,"221039","M8*45; ZK.TAPBOUT;RVS; A2","M8*45; ZK.TAPBOUT;RVS; A2",null,"0,003 kg"]
[2,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[2,"221066","M12*80; A2; ZK.RVS TAPBOUT","M12*80; A2; ZK.RVS TAPBOUT",null,"0,089 kg"]
[2,"223007","M12; ZK.MOER; RVS; A2","M12; ZK.MOER; RVS; A2",null,"0,017 kg"]
[10,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[4,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[16,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[4,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[1,"448547CC","RUBBER SCHRAPER DR-TROMMEL CC/TS.140","PLAAT 1500*200*6",null,"1,790 kg"]
[1,"448548CC","KLEMSTRIP RUBBER; L=1480; HOH.200","PLAAT 1480*35*3",null,"1,234 kg"]
[2,"448552CC","STELSTRIP STORTKLEP L=750","PLAAT 750*50*8",null,"2,283 kg"]
[2,"536748CC","BEV.BUIS STORTKLEP CC.142",null,null,"8,071 kg"]
[1,"539116CC","STORTKLEP; CC.142",null,null,"31,277 kg"]
[8,"536725CC","TROGSTELBEUGEL CC.142; 30°; RVS","TROGSTELBEUGEL CC.142; 30°; RVS",null,"20,131 kg"]
[1,"536728CC","DRIJFTROMMEL 288*1500; BEKLEED",null,null,"151,435 kg"]
[1,"536734CC","TROGSTELBEUGEL CC.142; 15°; RVS",null,null,"18,811 kg"]
[2,"536741CC","VERBINDINGSBRUG ZIJPLATEN CC.142; 1730",null,null,"13,740 kg"]
[1,"537920CC","SPANNER DRIJFTROMMEL CC.142; SNL ø55; L",null,null,"21,519 kg"]
[1,"537920CC_MIR","SPANNER DRIJFTROMMEL CC.142; RECHTS",null,null,"21,519 kg"]
[2,"538045CC","BORGAS SCHRAPER INWENDIG",null,null,"0,632 kg"]
[1,"539117CC","ZIJKANT CC.142; KOPSTUK; 5810",null,null,"117,407 kg"]
[1,"539117CC_MIR","ZIJKANT CC.142; KOPSTUK; 5810",null,null,"117,407 kg"]
[1,"518416CC","EINDSTUKL ONDERBAND CC.142; R",null,null,"961,745 kg"]
[2,"212009","M20; THVZ DRAADEIND; ISO; 8.8","M20; THVZ DRAADEIND; ISO; 8.8",null,"2,522 kg"]
[14,"217780","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART","LEIDINGKLEM ENKEL ø6; BOUTGAT M8; ZWART",null,"0,020 kg"]
[8,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[6,"221046","M10*20; ZK.TAPBOUT; RVS; A2","M10*20; ZK.TAPBOUT; RVS; A2",null,"0,025 kg"]
[58,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[2,"221063","M12*50; RVS ZK. TAPBOUT; A2","M12*50; RVS ZK. TAPBOUT; A2",null,"0,060 kg"]
[12,"221072","M16*35; ZK. RVS TAPBOUT; A2","M16*35; ZK. RVS TAPBOUT; A2",null,"0,093 kg"]
[4,"221243","M12*60; RVS ZK. BOUT; A2; DIN931","M12*60; RVS ZK. BOUT; A2; DIN931",null,"0,071 kg"]
[14,"221247","M12*90; RVS ZK. BOUT; A2","M12*90; RVS ZK. BOUT; A2",null,"0,095 kg"]
[2,"221253","M16*60; RVS ZK. BOUT; A2; DIN931","M16*60; RVS ZK. BOUT; A2; DIN931",null,"0,136 kg"]
[3,"221257","M16*80;ZK.RVS BOUT; A2","M16*80;ZK.RVS BOUT; A2",null,"0,163 kg"]
[18,"222244","M8*35;  A2;CIL.SCHR+BINNENZESK","M8*35;  A2;CIL.SCHR+BINNENZESK",null,"0,021 kg"]
[14,"223011","M20; ZK.MOER; RVS; A2","M20; ZK.MOER; RVS; A2",null,"0,065 kg"]
[26,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[60,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[15,"224462","M16; RVS BORGMOER; A2","M16; RVS BORGMOER; A2",null,"0,037 kg"]
[38,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[134,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[31,"225009","M16; RVS SLUITRING; A2; DIN125A","M16; RVS SLUITRING; A2; DIN125A",null,"0,012 kg"]
[6,"225024","M10; CARROS.SLUITRING; RVS; A2","M10; CARROS.SLUITRING; RVS; A2",null,"0,012 kg"]
[2,"225026","M16; CARROS. SLUITRING","M16; CARROS. SLUITRING",null,"0,042 kg"]
[8,"225028","M20; RVS SLUITRING; A2; M20*44*8;DIN7349","M20; RVS SLUITRING; A2; M20*44*8;DIN7349",null,"0,075 kg"]
[20,"225057","M12; RVS VEERRING; A2; DIN127","M12; RVS VEERRING; A2; DIN127",null,"0,004 kg"]
[2,"225059","M16; RVS VEERRING; A2","M16; RVS VEERRING; A2",null,"0,008 kg"]
[2,"243279","22212 EK; TONLAGER; SKF","22212 EK; TONLAGER; SKF",null,"1,150 kg"]
[2,"243530","SNL 512-610; LAGERHUIS; SKF","SNL 512-610; LAGERHUIS; SKF",null,"5,740 kg"]
[1,"243602","ASNH 512-610 EINDDEKSEL; SKF","ASNH 512-610 EINDDEKSEL; SKF",null,"0,120 kg"]
["1,500 ul","243632","TSNA 512 A; AFDICHTING; SKF","TSNA 512 A; AFDICHTING; SKF",null,"0,060 kg"]
["4,000 ul","243694","FRB 10/110; AFSTANDSRING; SKF","FRB 10/110; AFSTANDSRING; SKF",null,"0,246 kg"]
[2,"243702","H 312; TREKBUS; SKF","H 312; TREKBUS; SKF",null,"0,400 kg"]
[2,"246405","ZIJGELEIDEROL ø63.5*100; B","ZIJGELEIDEROL ø63.5*100; B",null,"0,998 kg"]
[9,"246416","TRANSPORTROL ø89*530; AS ø20*560","TRANSPORTROL ø89*530; AS ø20*560",null,"4,000 kg"]
[3,"246435","TRANSPORTROL ø89*1550; AS ø25*1581","TRANSPORTROL ø89*1550; AS ø25*1581",null,"16,889 kg"]
[20,"246580","TRANSPORTROL ø89*465; AS ø20*495","TRANSPORTROL ø89*465; AS ø20*495",null,"3,500 kg"]
[1,"400586FS","SMEERBOUT M16*40","SMEERBOUT M16*40",null,"0,099 kg"]
[1,"211804","1/8\"G-180º; SMEERNIPPEL","1/8\"G-180º; SMEERNIPPEL",null,"0,008 kg"]
[1,"400586FS","TAPBOUT THVZ. M16*40","TAPBOUT THVZ. M16*40",null,"0,092 kg"]
[1,"400591RT","BORGSCHIJF KA76; ø70*ø17*8","BORGSCHIJF KA76; ø70*ø17*8",null,"0,079 kg"]
[1,"400128RT","BORGSCHIJF ø70*ø13*8;  KA76","PLAAT ø70*8",null,"0,081 kg"]
[14,"404008TS","AFSTANDSBUS TROGSTELBEUGEL TS","BUIS ø21,3*2,65-54",null,"0,067 kg"]
[1,"405035CC","OPVULBUS ø70*ø50-20","BUIS ø70*10-20",null,"0,291 kg"]
[4,"405070TF","AS ø6-3000","AS ø6-3000",null,"0,681 kg"]
[1,"405210TS","OPVULBUS ø30*ø16,5*20,5","AS ø30-20,5",null,"0,081 kg"]
[2,"406253TS","DRAADSPIL M20*750; THVZ","DRAADSPIL M20*750; THVZ",null,"1,851 kg"]
[4,"406316CC","DRAADBUS TROGSTELBEUGEL BEGIN/EIND","AS ø20-54",null,"0,101 kg"]
[1,"448548CC","KLEMSTRIP RUBBER; L=1480; HOH.200","PLAAT 1480*35*3",null,"1,234 kg"]
[1,"449184CC","RUBBER SCHRAPER DR-TR CC.142; 1500*400","PLAAT 1500*400*6",null,"3,596 kg"]
[2,"449350CC","BORGPLAAT STORTSCHOT CC.140","PLAAT 80*65*5",null,"0,085 kg"]
[1,"450871CC","SCHUIFBLOK REACTIEARM","PLAAT 115*30*12",null,"0,136 kg"]
[1,"467181CC","SCHRAPER KEERTROMMEL CC/TS.140","PLAAT 1600*264*4",null,"13,204 kg"]
[1,"467185CC","SCHRAPER DRIJFTROMMEL UITW; CC/TS.140","PLAAT 1743*116*5",null,"7,632 kg"]
[6,"467187CC","STEUNROLHOUDER CC.142","PLAAT 190*136*5",null,"0,868 kg"]
[2,"467210CC","STEUN GELEIDING STORTSCHOT CC.142","PLAAT 433*79*5",null,"0,859 kg"]
[2,"467212CC","BEV.BEUGEL ZIJGELEIDEROL CC.142","PLAAT 189*65*10",null,"0,904 kg"]
[2,"467217CC","BEV.STEUN TROGSTELBEUGEL STUREN CC.142","PLAAT 160*152*8",null,"1,177 kg"]
[1,"467876CC","ONDERSTEUNINGSPROFIEL RUBBER SCHRAPER CC.142","PLAAT 1490*181*3",null,"6,472 kg"]
[1,"469048CC","BEV.STEUN SCHRAPER DRIJFTR CC.142; R","PLAAT 280*267*6",null,"1,397 kg"]
[1,"469048CC_MIR","BEV.STEUN SCHRAPER DRIJFTR CC.142; L","PLAAT 280*267*6",null,"1,397 kg"]
[1,"469070CC_MIR","REACTIEARM KA77","PLAAT 858*170*10",null,"6,913 kg"]
[1,"516338CC","TROGSTELBEUGEL CC.142; 10°; STUREN; KPL",null,null,"13,965 kg"]
[4,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[4,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[4,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[2,"467226CC","KLEMPLAAT DRAAGROL STUREN CC","PLAAT 148*60*5",null,"0,097 kg"]
[1,"536754CC","TROGSTELBEUGEL CC.142; 10°; STUREN",null,null,"13,664 kg"]
[1,"517537CC","SCHRAPER INWENDIG CC.142",null,null,"15,029 kg"]
[13,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[13,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[26,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[1,"451226CC","SCHRAAPSTRIP L=1650","PLAT 100*10-1650",null,"1,072 kg"]
[2,"469328CC","KLEMPROFIEL SCHRAAPSTRIP","PLAAT 1650*109*4",null,"5,780 kg"]
[2,"538117CC","BEVESTIGINGSPROFIEL SCHRAPER",null,null,"1,016 kg"]
[1,"518330CC","STORTKLEP ONDERBAND CC.142; KPL",null,null,"55,681 kg"]
[2,"218001","INSTEEKDOP ø42*1.3/3","INSTEEKDOP ø42*1.3/3",null,"0,009 kg"]
[8,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[2,"221039","M8*45; ZK.TAPBOUT;RVS; A2","M8*45; ZK.TAPBOUT;RVS; A2",null,"0,003 kg"]
[2,"221060","M12*35; RVS ZK. TAPBOUT; A2","M12*35; RVS ZK. TAPBOUT; A2",null,"0,049 kg"]
[2,"221066","M12*80; A2; ZK.RVS TAPBOUT","M12*80; A2; ZK.RVS TAPBOUT",null,"0,089 kg"]
[2,"223007","M12; ZK.MOER; RVS; A2","M12; ZK.MOER; RVS; A2",null,"0,017 kg"]
[10,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[4,"224460","M12; RVS BORGMOER; A2","M12; RVS BORGMOER; A2",null,"0,019 kg"]
[16,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[4,"225007","M12; RVS SLUITRING; A2; DIN125A","M12; RVS SLUITRING; A2; DIN125A",null,"0,006 kg"]
[1,"448547CC","RUBBER SCHRAPER DR-TROMMEL CC/TS.140","PLAAT 1500*200*6",null,"1,790 kg"]
[1,"448548CC","KLEMSTRIP RUBBER; L=1480; HOH.200","PLAAT 1480*35*3",null,"1,234 kg"]
[2,"448552CC","STELSTRIP STORTKLEP L=750","PLAAT 750*50*8",null,"2,283 kg"]
[2,"536748CC","BEV.BUIS STORTKLEP CC.142",null,null,"8,071 kg"]
[1,"539116CC","STORTKLEP; CC.142",null,null,"31,277 kg"]
[8,"536725CC","TROGSTELBEUGEL CC.142; 30°; RVS","TROGSTELBEUGEL CC.142; 30°; RVS",null,"20,131 kg"]
[1,"536728CC","DRIJFTROMMEL 288*1500; BEKLEED",null,null,"151,435 kg"]
[1,"536734CC","TROGSTELBEUGEL CC.142; 15°; RVS",null,null,"18,811 kg"]
[1,"536741CC","VERBINDINGSBRUG ZIJPLATEN CC.142; 1730",null,null,"13,740 kg"]
[1,"537920CC","SPANNER DRIJFTROMMEL CC.142; SNL ø55; L",null,null,"21,519 kg"]
[1,"537920CC_MIR","SPANNER DRIJFTROMMEL CC.142; RECHTS",null,null,"21,519 kg"]
[2,"538045CC","BORGAS SCHRAPER INWENDIG",null,null,"0,632 kg"]
[1,"539117CC","ZIJKANT CC.142; KOPSTUK; 5810",null,null,"117,407 kg"]
[1,"539117CC_MIR","ZIJKANT CC.142; KOPSTUK; 5810",null,null,"117,407 kg"]
[6,"536731CC","OPHANGSTEUN ONDERBAND CC.142",null,null,"7,368 kg"]
[4,"536737CC","OPHANGSTEUN ONDERBAND CC.142; KOP",null,null,"8,956 kg"]
[1,"536740CC","MEENEMER VLAKKABEL CC; ONDERBAND; 560",null,null,"3,105 kg"]
[1,"518682CC","ELEKTRISCH SYSTEEM CC.142-501420CC",null,null,"235,992 kg"]
[1,"518688CC","VLAKKABELRAIL CC.142-501420CC",null,null,"235,992 kg"]
[1,null,"TREKKOORDSCHAKELAAR 440E-L22BNSMNH ","TREKKOORDSCHAKELAAR 440E-L22BNSMNH ",null,"0,365 kg"]
[1,"215728","D-SLUITING; M4; RVS","D-SLUITING; M4; RVS",null,"0,009 kg"]
[10,"218007","M8; OOGMOER; RVS; DIN 582","M8; OOGMOER; RVS; DIN 582",null,"0,046 kg"]
[10,"221035","M8*25; ZK.TAPBOUT; RVS, A2","M8*25; ZK.TAPBOUT; RVS, A2",null,"0,016 kg"]
[10,"225023","M8; RVS CARROS.SLUITRING A2","M8; RVS CARROS.SLUITRING A2",null,"0,005 kg"]
[1,"247347 L=42500","TREKKOORD ","STAALKABEL; 6*7+1; GG; PVC ROOD; L=36 mtr",null,"4,198 kg"]
[1,"247561","SPANSCHROEF 2* OOG; M6; RVS; DIN1480","SPANSCHROEF 2* OOG; M6; RVS; DIN1480",null,"0,074 kg"]
[1,"223004","M6; ZK.MOER; RVS; A2","M6; ZK.MOER; RVS; A2",null,"0,002 kg"]
[1,"247561-1",null,null,null,"0,034 kg"]
[2,"247561-2",null,"AS ø6-50",null,"0,019 kg"]
[18,"265001","RAILPROFIEL 023200-4","RAILPROFIEL 023200-4",null,"6,216 kg"]
[16,"265002","RAILVERBINDER C-RAIL; 23210","RAILVERBINDER C-RAIL; 23210",null,"0,274 kg"]
[43,"265006","KABELWAGEN; LANG; 23263; THVZ","KABELWAGEN; LANG; 23263; THVZ",null,"0,486 kg"]
[2,null,"M6*80; RVS SLOTBOUT; A2; DIN603","M6*80; RVS SLOTBOUT; A2; DIN603",null,"0,022 kg"]
[4,"404206FO","KOGELLAGER ø25*ø8*7",null,null,"0,024 kg"]
[1,"405138CO",null,"AS ø50-80",null,"0,057 kg"]
[1,"448823CO",null,"PLAAT 80*30*2",null,"0,036 kg"]
[1,"536872CO",null,null,null,"0,252 kg"]
[1,"536872CO",null,null,null,"0,252 kg"]
[54,"515521CC","RAILHOUDER VLAKKABEL; IPE100; RVS",null,null,"0,466 kg"]
[2,"221036","M8*30; ZK.TAPBOUT; RVS; A2","M8*30; ZK.TAPBOUT; RVS; A2",null,"0,018 kg"]
[2,"224458","M8; RVS BORGMOER; A2","M8; RVS BORGMOER; A2",null,"0,006 kg"]
[2,"225005","M8; RVS SLUITRING; A2; DIN125A","M8; RVS SLUITRING; A2; DIN125A",null,"0,002 kg"]
[1,"446258CC","BEVESTIGINGSPLAAT RAILHOUDER","PLAAT 100*40*3",null,"0,093 kg"]
[1,"465308CC","BORGPLAAT RAILHOUDER","PLAAT 120*40*3",null,"0,113 kg"]
[2,"465309CC","KLEMPLAAT RAILPROFIEL","PLAAT 68*40*3",null,"0,065 kg"]
[2,"465310CC","KIKKERPLAAT RAILHOUDER","PLAAT 87*40*3",null,"0,038 kg"]
[1,"518353CC","MONTAGEPLAAT HEA260",null,null,"3,051 kg"]
[4,"221027","M6*40; ZK.TAPBOUT; RVS; A2","M6*30; ZK.TAPBOUT; RVS; A2",null,"0,012 kg"]
[1,"468302CC","MONTAGEPLAAT KOPPELKAST 260*160; HEA260","PLAAT 342*330*4",null,"3,005 kg"]