{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Blad1"],"not_rendered":{"charts":0,"images":12,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Blad1","index":0,"n_rows":11,"n_cols":4,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
[2,"515507CC","LOOPROL SCHUIFBAND AANGEDREVEN; KPL"]
[1,"404048CC","AS LOOPROL SCHUIFBAND","AS ø40-43"]
[1,"535594CC","LOOPROL SCHUIFBAND AANGEDREVEN"]
[1,"404046CC",null,"PLAAT ø126*10"]
[1,"404047CC",null,"AS ø100-30"]
[1,"243060","KOGELLAGER 6207-2RS1; RVS KOGELLAGER","KOGELLAGER 6207-2RS1; RVS KOGELLAGER"]
[1,"225011","M20; RVS SLUITRING; A2; DIN125A","M20; RVS SLUITRING; A2; DIN125A"]
[1,"225061","M20; VEERRING; RVS; A2","M20; VEERRING; RVS; A2"]
[1,"221085","M20*50; ZK.RVS.TAPBOUT; A2","M20*50; ZK.RVS.TAPBOUT; A2"]
[1,"225425","ASBORGRING ø35; RVS","ASBORGRING ø35; RVS"]
[1,"225558","GATBORGRING; G72; RVS","GATBORGRING; G72; RVS"]