{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Chart1","Visco"],"not_rendered":{"charts":2,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[{"sheet":"Chart1","index":0,"reason":"not_a_worksheet"}],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Visco","index":1,"n_rows":32,"n_cols":11,"rows_kept":32,"cut":false,"hidden":false,"merged":[[6,5,8,5],[6,6,8,6]]}
[]
["CB Calculator vanuit de dynamische viscositeit"]
[]
["Volgorde","Visco letter","Ref (mPas)",null,"Geef de dynamische viscositeit in, en druk op bereken:",null,null,null,null,9800,"mPas"]
[1,"Z2",25118,null,null,"Geef het aantal kilo's af te werken chocolade in:",null,null,null,1000,"kg"]
[2,"Z1",20931]
[3,"Z",17443,null,null,"W",-0.21166306695464362]
[4,"Y",14536]
[5,"X",12113]
[6,"W",10094,"<="]
[7,"V",8705]
[8,"U",7010,null,null,null,null,"Afwerken op visco "]
[9,"T",5740]
[10,"S",4760,null,null,"Afwerken op visco ",null,17,{"$f":"MATCH(F7,B5:B32,0)","v":6}]
[11,"R",3990]
[12,"Q",3390]
[13,"P",2905]
[14,"O",2515]
[15,"N",2197]
[16,"M",1935,null,null,"Boter toe te voegen=:",null,{"$f":"J5*H21/100","v":107.88336933045355},"kg"]
[17,"L",1719,null,null,null,null,{"$f":"H14-I14+G7","v":10.788336933045356},"%"]
[18,"K",1540]
[19,"J",1388]
[20,"I",1261]
[21,"H",1152]
[22,"G",1059]
[23,"F",979]
[24,"E",906.48148148148141]
[25,"D",839.33470507544564]
[26,"C",777.16176395874595]
[27,"B",719.5942258877277]
[28,"A",666.29094989604414]